# Continuous Cartogram

## Documentation for package ‘cartogramR’ version 1.5-1

- DESCRIPTION file.
- User guides, package vignettes and other documentation.

## Help Pages

as.sf | Coerce an object to a sf object
as.sf.cartogramR | Coerce a cartogramR to a sf object
as.sfc | Coerce an object to a sfc object
as.sfc.cartogramR | Coerce a cartogramR to a sfc object
as.sfmultipolygon | Transform a sf object with several rows (polygons) by region to an sf object with one row by region and thus one multipolygon by region
cartogramR | Make a continuous cartogram (density equalizing maps)
cartogramR_options | Set the options of cartogramR in the correct format
check_ring_dir | Polygon rings directions are checked and corrected if asked.
dist_between_vertices | Analyse some of the grid options
france_dept | Map of the population of mainland France (year 2018)
france_rivers | Map of french rivers of mainland France
from_coord_polygon | Transform from coordinates system used in the polygons to coordinates system used in flow based cartogram
grid_analysis | Analyse some of the grid options
make_layer | Make a layer
plot.cartogramR | Plot a cartogram object
plot.dbv.cartogramR | Plot a dbv.cartogram object
plot.gridanalysis.cartogramR | Plot a gridanalysis.cartogram object
precartogramR | Make a pre cartogram analysis
print.cartogramR | Print a cartogram object
print.summary.cartogramR | Print a summary of a cartogram object
residuals.cartogramR | Errors of a cartogram object
summary.cartogramR | Summary of a cartogram object
summary.dbv.cartogramR | Summary of a dbv.cartogram object
summary.gridanalysis.cartogramR | Summary of a gridanalysis.cartogram object
to_coord_polygon | Transform from coordinates system used in flow based cartogram to coordinates system used in the polygons
usa | Map of the number of electors in each state of the USA
warp_features | Apply the deformation used to build a cartogram to a set of simple geometry coordinates